[bookmark: _Toc536525950]ENQUIRY FOR PREQUALIFICATION (NO.PRQ/JPT/40
/26)
STRUCTURES A & E, MELLITAH COMPLEX EXPANSION & CO2 MANAGEMENT INTEGRATED DEVELOPMENT PROJECT


[bookmark: _Hlk152846297]SUPPLY REQUISITION FOR 16” SEAMLESS CARBON STEEL PIPES FOR CO2 INJECTION FROM MELLITAH TO SABRATHA (WP4B2)

Mellitah Oil & Gas B.V. (MOG) intends to enhance its production by adding new offshore and onshore production facilities, under STRUCTURES A & E, MELLITAH COMPLEX EXPANSION & CO2 Management Integrated Development Project. The Overall Development will be implemented on individual projects basis; including Supply Requisition for 16” Seamless Carbon Steel Pipes for Co2 Injection from Mellitah to Sabratha related to the CO2 Management (WP4B2). MOG would like to invite the interested Contractors who are qualified and experienced in Seamless Carbon Steel Pipes to express their interest to participate in the Tender of Supply requisition, by submitting a Prequalification request to Company. Information about the Project and the Participation requirements are detailed here following. 

PROJECT DESCRIPTION

The overall A & E structures development project foresees the exploitation of Structures A and E located in the Libyan offshore area of NC 41 Block. The “A” Structure is in the central-western part of the area, approximately 80 Km from Libyan coast, where water depth is ranges between 95 and 105 m. While, “E” Structure is located in the central-eastern part of the area, about 130 Km far from the Libyan coast, in a water depth ranging from 205 to 235 m.

The selected offshore development scenario foresees:

· EPIC for Production Platform E (PPE) (WP1): A New Production Platform installed in 220 m water depth (outside the scope of this pre-qualification)
· EPIC for Wellhead Production Fixed Platform A (WHPA) (WP2): A New Wellhead Platform installed in 96m water depth (outside the scope of this pre-qualification)
· EPIC for Modification of Existing Sabratha Fixed Platform (WP3) (outside the scope of this pre-qualification).
· EPIC for WHPA to Sabratha Sealines and Subsea Systems (WP4A) (outside the scope of this pre-qualification).
· EPIC for Sealines and Subsea system for structure E and CO2(WP4B1): Risers (for connections to PPE), Sealines and Subsea system (outside the scope of this pre-qualification). 
· Supply of seamless carbon steel pipes for CO2 injection from MCX to Sabratha platform (WP4B2): (Inside the scope of this pre-qualification, free issued or Novated to WP4B1). Please refer to “SCOPE OF WORK” section for further details.
· EPC for Subsea Production Systems (SPS) for Structure E and CO2 (WP4B3): (outside the scope of this pre-qualification, free issued or Novated to WP1 / WP4B1)
· The onshore development scenario foresees upgrade of the existing onshore Mellitah Complex (WP5) (outside the scope of this pre-qualification).
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SCHEDULE  
The SCOPE OF SUPPLY execution is expected to start by Q2 2027 and to be completed by Q3 2028.
Associated Tendering process is planned to occur from Q4 2026 to Q1 2027.

SCOPE OF WORK
CONTRACTOR SHALL supply the Carbon Steel line pipes, mother pipe and bends for the new 16” CO2 pipeline from Mellitah Complex plant to Sabratha platform (including subsea spools and onshore section to insulating joint and anticorrosion coating for CO2 injection line pipe and Topside and Riser Pipes and Bends for CO2 injection) in the “A&E, Mellitah Complex Expansion & CO2 Management Integrated Development Project”. 

The Scope of Work includes, as a minimum, project management, engineering required for the supply, procurement of raw materials, manufacture, qualification, inspection and testing, anticorrosion coating, certification, documentation, preservation, handling and delivery of the following items:

· Supply of seamless carbon steel pipes for CO2 injection (WP4B2) (free issue or novated to WP4B1):

· Supply of the 16’’ Seamless Carbon Steel Line Pipes, mother pipe and bends to be coated by anticorrosion coating to fabricate the 16” CO2 pipeline from Mellitah Complex plant to Sabratha platform and associated spools including Subsea Offshore Pipeline and Spools and Onshore Pipeline section (~ 110 Km) to be delivered at load out location for being picked up by WP4b1 . Concrete coating onshore side is Out of the Scope (~5 km) and will be done by WP4b1.
· Supply of uncoated Topside and Riser Pipes and Bends for CO2 injection to be delivered to WP4B1 (Optional).
· Certificates Type 3.2 (as per EN 10204:2004) are required for final pipes and bends.

The above SoW includes all related functions, activities and services of each and every kind to accomplish the work, including as minimum; management, supervision, quality assurance, quality control, training, produce as-built drawings/documentation, compile record books, material handling/expediting, preservation, cost control, scheduling, status/progress reporting, interface with Certifying Authority, interfacing with related facilities both Existing and New, interface management in general,  provide all labour, resources, tools, equipment, plant, consumables, spares, vendor specialist assistance, accommodation and related infrastructure elements, and  implement  all safety and environmental requirements.
The following work categories shall be part of the scope of work:

· HEALTH, SAFETY, ENVIRONMENT AND QUALITY MANAGEMENT SYSTEMS 

· PROJECT MANAGEMENT

· ENGINEERING

· PROCUREMENT SERVICES

· MANUFACTURING, INSPECTION AND TESTING

· CERTIFICATION, APPROVALS, CONSENTS AND PERMITS


IMPORTANT
The Applicant shall provide, during the Pre-Qualification phase, Third Party certification or documented Third Party qualification evidence demonstrating the applicability of SMLS line pipes for dense-phase 16” CO2 transportation, supported by relevant full-scale testing.

The Applicant shall identify the activities to be performed directly and shall nominate the proposed subcontractors for any major or significant part of the Scope of Work requiring qualification at this stage.
In case of Consortium, a consortium agreement shall be provided (identify lead partner, financial responsibility split, liability allocation, decision‑making preliminary rules).

It is required that the main core work shall be executed by the Applicant.

Only original manufacturers with proven capability and experience in the manufacture and supply of seamless carbon steel line pipes for comparable oil and gas pipeline applications will be considered for the Scope of Work described above.

The Applicant shall demonstrate strong HSE and Quality performance factors in similar projects and provide their commitment to ensuring that all conducted on their behalf are carried out in a safe and efficient manner. 

The Applicant shall provide a detailed reference list of previously manufactured and supplied seamless carbon steel line pipes of comparable characteristics, indicating the client/project, application, pipe diameter, wall thickness, material grade, applicable standard, supplied quantity or length, manufacturing mill and year of supply.

The Applicant shall provide a preliminary manufacturing and delivery schedule for the requested supply.
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